

Image 1: The pivot doors from Hörmann create a reduced profile view without a door frame and are particularly suitable for wide passageways.

Minimalist design without door frames

Elegant pivot doors from Hörmann

**Hörmann is expanding its range of steel loft doors to include pivot doors and is setting new standards in minimalist door design. This special form of a hinged door creates a reduced profile view without a door frame and is particularly suitable for wide passageways in living and business rooms. The door leaves are attached to hinges in the floor and to the ceiling or lintel and swing on a vertical axis in both directions. This innovative design allows for maximum transparency and light-flooded rooms, while the filigree glazing beads provide an elegant accent.**

Hörmann's exclusive pivot doors are a particularly elegant solution for wide passageways in living and business rooms. Even when closed, they ensure maximum transparency and light-flooded rooms. The doors have a high-quality appearance and can be combined with many furnishing styles, while their design makes them a real eye-catcher. They are supplied with the Slim glazing bead as standard, thus creating a minimalist profile look. This look is enhanced by the design of the hinged door as a pivot door. The door leaf is anchored directly to the floor, ceiling or lintel by hinges. The door swings easily in both directions on this vertical axis. The pivot point can be individually determined. This type of installation does not require a door frame, which saves space at the side and contributes to a minimalist look. The pivot doors have a maximum door leaf width of 2000 mm and a height of up to 3000 mm. They are used in passageways where double-leaf doors or doors with side elements would otherwise be required. Thanks to the same door styles and rail arrangement, the pivot doors harmonise perfectly with the hinged doors from the Hörmann steel loft door range.

The pivot doors and the optionally available side elements are supplied as standard in Jet black matt. There is also a choice of five preferred colours – Anthracite grey, White or Grey aluminium, Traffic white and Anthracite metallic – as well as RAL colours of your choice, special NCS colours and textured and pearl effect colours.

(2184 characters incl. spaces)

**Images and captions:**



**Image 2:** The door leaf of the Hörmann pivot doors is anchored directly to the floor, ceiling or lintel by hinges. The door swings easily and elegantly in both directions on this vertical axis.



**Image 3:** Thanks to the same door styles and rail arrangement, the pivot doors harmonise optimally with the Hörmann steel loft doors as a hinged or sliding door variant.

Photos: Hörmann